{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / 3AMXF-A9"]
[]
[]
[]
[]
["","","","","ATXF25A5V1B / ATXF25A5V1B / ATXF25A5V1B / 3AMXF52A2V1B9"]
["Холодопроизводительность","Мин.","","кВт","1.8"]
["","Ном.","","кВт","5.2"]
["","Макс.","","кВт","7"]
["Теплопроизводительность","Мин.","","кВт","1.3"]
["","Ном.","","кВт","6.8"]
["","Макс.","","кВт","8"]
["Номинальная эффективность","EER","","","4.05"]
["","COP","","","3.88"]
["","Годовое потребление энергии","","кВтч","642"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++"]
["","Производительность","Pрасч.","кВт","5.2"]
["","SEER","","","7.2"]
["","Годовое потребление энергии","","кВтч/г","253"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+"]
["","Производительность","Pрасч.","кВт","5"]
["","SCOP/A","","","4.01"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.74"]
["","Годовое потребление энергии","","кВтч/г","1744"]