{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Холодопроизводительность","Мин.","","kW","","","1.40"]
["","Макс.","","kW","","","4.00"]
["","Ном.","","kW","","","3.40"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","A"]
["","","Нагрев","","","","A"]
["Теплопроизводительность","Ном.","","kW","","","4.00"]
["","Мин.","","kW","","","1.40"]
["","Макс.","","kW","","","5.20"]
["Примечания","","","","","","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","(3) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","","(4) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["Холодопроизводительность","Мин.","","кВт","1.30","1.30","","1.40"]
["","Ном.","","кВт","2.50","2.50","","3.40"]
["","Макс.","","кВт","3.20","3.20","","4.00"]
["Теплопроизводительность","Мин.","","кВт","1.30","1.30","","1.40"]
["","Ном.","","кВт","2.80","2.80","","4.00"]
["","Макс.","","кВт","4.70","4.70","","5.20"]
["Номинальная эффективность","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Годовое потребление энергии","","кВтч","278","278","","402"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","","A"]
["","","Нагрев","","A","A","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A+++","A+++","","A+++"]
["","Производительность","Pрасч.","кВт","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Годовое потребление энергии","","кВтч/г","102","102","","139"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+++","A+++","","A+++"]
["","Производительность","Pрасч.","кВт","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh Теплопроизводительность при -10°","","кВт","2.30","2.30","","2.35"]
["","Годовое потребление энергии","","кВтч/г","659","659","","686"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]