{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BAEF125AWB"]
[]
[]
[]
[]
["","","","","BAEF125AWB."]
["Потребляемая мощность","кВт","","","0.006"]
["Корпус","Цвет","","","Gray"]
["","СИД работы","Цвет","","Blue/red"]
["Размеры","Блок","Высота","мм","100"]
["","","Ширина","мм","840"]
["","","Глубина","мм","840"]
["","Упакованный блок","Высота","мм","168"]
["","","Ширина","мм","910"]
["","","Глубина","мм","910"]
["Масса","Блок","","кг","12.0"]
["","Упакованный блок","","кг","15.5"]
["Упаковка","Материал","","","Тонкий картон"]
["","Вес","","кг","4"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50/60"]
["","Напряжение","","V","220-240/220"]
["Примечания","","","","(1) - С 2 датчиками (коэффициент регулирования 0,65): A+; Другое: A"]