{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":21,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CI-B"]
[]
[]
[]
[]
["","","","","","GCI2010B3B1D4R","HCI2015B2B1D4R","HCI2018B2B1D4R","GCI2020B3B1D4R","HCI2020B2B1D4R","GCI2022B3B1D4R","GCI2030B3B1D4R","HCI2030B2B1D4R","GCI2040B3B1D4R","GCI3050B3B1D4R","HCI2050B2B1D4R","GCI3060B3B1D4R","HCI3060B2B1D4R","GCI4120B3B1D4R","HCI4120B2B1D4R","HCI4140B2B1D4R"]
["Холодопроизводительность","Среднетемп. режим","R-134a","Ном.","кВт","2.913","","","4.046","","5.012","7.167","","9.263","11.255","","13.417","","18.253"]
["Корпус","Цвет","","Конденсаторный блок","","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый"]
["","Материал","","Конденсаторный блок","","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь","Сталь"]
["Размеры","Конденсаторный блок","","Ширина","мм","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,404","1,684","1,684","1,684"]
["","","","Толщина","мм","747","747","747","747","747","747","747","747","747","548","747","548","548","748","748","748"]
["Компрессор","Количество","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Тип","","","","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный","Полугерметичный"]
["","Модель","","","","2HES‐1Y","2GES-2Y","2FES-2Y","2FES-2Y","2DES‐2Y","2EES‐2Y","2CES‐3Y","4FES-3Y","4EES‐4Y","4DES-5Y","4DES-5Y","4CES-6Y","4CES-6Y","4PES-12Y","4PES-12Y","4NES-14Y"]
["","Способ запуска_","","","","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением","С инверторным управлением"]
["Конденсатор","Воздушный поток","","","м³/ч","2,943","2,943","2,943","2,943","2,943","2,943","2,701","2,701","2,701","5,850","2,701","5,850","5,850","5,366","5,366","5,366"]
["Рабочий диапазон","Температура окружающей среды","","Мин.","°С","20","20","20","20","20","20","20","20","20","20","20","20","20","20","20","20"]
["","","","Макс.","°С","45","45","45","45","45","45","45","45","45","45","45","45","45","45","45","45"]
["Хладагент","Тип","","","","R-134a","R-449A","R-449A","R-134a","R-449A","R-134a","R-134a","R-449A","R-134a","R-134a","R-449A","R-134a","R-449A","R-134a","R-449A","R-449A"]
["","ПГП","","","","1,430","1,397","1,397","1,430","1,397","1,430","1,430","1,397","1,430","1,430","1,397","1,430","1,397","1,430","1,397","1,397"]
["Стандартный ресивер жидкости","л","","","","5.7","2.3","2.3","5.7","5.7","5.7","5.7","5.7","10","10","5.7","10","10","21","21","21"]
["Уровень звукового давления","Ном.","","","дБA","33","34","35","34","36","35","35","37","39","40","40","41","42","42","45","48"]
["Электропитание","Напряжение","","","V","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400","380-400"]
["","Фаза","","","","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Частота","","","Гц","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]