{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYT-CZO"]
[]
[]
[]
[]
["","","","","","EWYT021CZO-A1","EWYT032CZO-A1","EWYT040CZO-A1","EWYT064CZO-A2"]
["Размеры","Блок","","Высота","мм","1,878","1,878","1,878","1,878"]
["","","","Ширина","мм","1,152","1,752","1,752","2,906"]
["","","","Глубина","мм","802","802","802","814"]
["Масса","Блок","","","кг","265","357","357","620"]
["Уровень звуковой мощности","Охлаждение","","Ном.","дБA","76.0","79.0","80.0","83.0"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","59.6","62.2","63.2","65.4"]
["Хладагент","ПГП","","","","675.0","675.0","675.0","675.0"]
["","Заправка","","","tCO2Eq","4,928.0","6,422.0","6,635.0","11,255.0"]
["","Заправка","","","кг","7.3","9.5","9.8","16.6"]
["Подсоединение труб","Жидкость","","НД","мм","28.6","28.6","28.6","28.6"]
["","Газ","","НД","мм","9.52","12.7","12.7","12.7, 9.52"]
["Подсоединения труб","перепад уровня","IU - OU","Макс.","м","10.0","10.0","10.0","10.0"]
["Электропитание","Частота","","","Гц","50","50","50","50"]