{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Холодопроизводительность","Мин.","","kW","1.7"]
["","Макс.","","kW","6.5"]
["","Ном.","","kW","6.0 (2)"]
["Подсоединение труб","Жидкость","НД","мм","6.35"]
["","Газ","НД","мм","12.7"]
["","Дренаж","НД","мм","VP20 (внешний диам.26, внутр. диам. 20)"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,030"]
["","EER","","","2.91 (1)"]
["","COP","","","3.21 (1)"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","C"]
["","","Нагрев","","C"]
["Теплопроизводительность","Ном.","","kW","7.0 (3)"]
["","Мин.","","kW","1.7"]
["","Макс.","","kW","8.0"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Охлаждение: темп. в помещении: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5 м"]
["","","","","(3) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м"]
["","","","","(4) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]