{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L8Y1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L8Y1B","FHQ125CAVEB / RZQSG125L8Y1B"]
["Охлаждение помещений","SEER","","","5.1","5.1","5.61"]
["","Годовое потребление энергии","","кВтч/г","652","652","749"]
["","Производительность","Pрасч.","кВт","9.5","9.5","12"]
["","Класс энергоэффективности","","","B","B","A+"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","7.6","7.6","7.6"]
["","SCOP/A","","","3.8","3.8","4.01"]
["","Класс энергоэффективности","","","A","A","A+"]
["","Годовое потребление энергии","","кВтч/г","2,800","2,800","2,654"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["Холодопроизводительность","Ном.","","кВт","","","12.0"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","","","2,075"]
["","EER","","","","","2.89"]
["","COP","","","","","3.62"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","C"]
["","","Нагрев","","","","A"]
["Теплопроизводительность","Ном.","","кВт","","","13.5"]
["Примечания","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]