{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","","","","","0.029","","0.032"]
["","Hагрев","","Ном.","кВт","","","","","0.032","","0.035"]
["Корпус","Цвет","","","","","","","","Белый","","Белый"]
["Размеры","Блок","","Высота","мм","","","","","295","","295"]
["","","","Ширина","мм","","","","","990","","990"]
["","","","Глубина","мм","","","","","263","","263"]
["Масса","Блок","","","кг","","","","","13.5","","13.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","","","","16.8","","17.3"]
["","","","Medium","м³/мин","","","","","14.4","","14.8"]
["","","","Низк.","м³/мин","","","","","11.9","","12.2"]
["","","","Тихая работа","м³/мин","","","","","10.5","","10.7"]
["","","Нагрев","Выс.","м³/мин","","","","","17.3","","17.9"]
["","","","Medium","м³/мин","","","","","14.8","","15.8"]
["","","","Низк.","м³/мин","","","","","12.2","","12.8"]
["","","","Тихая работа","м³/мин","","","","","10.7","","11.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","","","","59","","62"]
["","Отопление","","","дБA","","","","","61","","62"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","","","","","43","","46"]
["","","","Medium","дБA","","","","","39","","42"]
["","","","Низк.","дБA","","","","","34","","37"]
["","","","Тихая работа","дБA","","","","","31","","34"]
["","Hагрев","","Выс.","дБA","","","","","42","","45"]
["","","","Средн.","дБA","","","","","38","","41"]
["","","","Низк.","дБA","","","","","33","","36"]
["","","","Тихая работа","дБA","","","","","30","","33"]
["Подсоединение труб","Жидкость","","НД","мм","","","","","6.35","","6.35"]
["","Газ","","НД","мм","","","","","12.7","","12.7"]
["","Дренаж","","","","","","","","18","","18"]
["Control systems","Infrared remote control","","","","","","","","ARC470A1","","ARC470A1"]
["","Wired remote control","","","","","","","","BRC073A1","","BRC073A1"]
["Стандартные аксессуары","Сухие батареи AAA","","","","","","","","2","","2"]
["","Инструкции по установке","","","","","","","","1","","1"]
["","Руководство по эксплуатации","","","","","","","","1","","1"]
["","Пульт дистанционного управления","","","","","","","","1","","1"]
["","Держатель пульта дистанционного управления","","","","","","","","1","","1"]
["","Монтажная пластина","","","","","","","","1","","1"]
["","Крепежные винты внутреннего блока","","","","","","","","2","","2"]
["Power supply","Наименование","","","","","","","","V1","","V1"]
["","Фаза","","","","","","","","1~","","1~"]
["","Частота","","","Гц","","","","","50","","50"]
["","Напряжение","","","В","","","","","220-240","","220-240"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.023","0.023","0.029","0.040","","0.032"]
["","Hагрев","","Ном.","кВт","0.023","0.023","0.029","0.040","","0.035"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","286","286","286","286","","295"]
["","","","Ширина","мм","770","770","770","770","","990"]
["","","","Глубина","мм","225","225","225","225","","263"]
["Масса","Блок","","","кг","8","8","8.5","9.00","","13.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.8","10","11.5","12.6","","17.3"]
["","","","Средн.","м³/мин","8","8","8","9","","14.8"]
["","","","Низк.","м³/мин","6","6.2","6.4","6.9","","12.2"]
["","","","Тихая работа","м³/мин","4.3","4.3","4.4","4.9","","10.7"]
["","","Hагрев","Выс.","м³/мин","10.4","10.4","11.9","12.8","","17.9"]
["","","Нагрев","Средн.","м³/мин","8.3","8.4","8.6","8.8","","15.8"]
["","","Hагрев","Низк.","м³/мин","6.2","6.4","6.5","6.7","","12.8"]
["","","","Тихая работа","м³/мин","5.3","5.3","5.3","5.2","","11.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","53","54","54","59.0","","60"]
["","Отопление","","","дБA","55","55","56","59.0","","62"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","39","40","43","45.0","","45"]
["","","","Средн.","дБA","33","33","34","36.0","","41"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","26","27","30.0","","36"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","20","20","20","22.0","","33"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","40","40","44.0","","44"]
["","Нагрев","","Средн.","дБA","34","34","35","34.0","","40"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","28","28","29","28.0","","35"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","21","21","21","22.0","","32"]
["Подсоединение труб","Жидкость","","НД","мм","6","6","6","6","","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","9.50","","12.7"]
["","Дренаж","","","","18","18","18","18","","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","","1~"]
["","Частота","","","Гц","50","50","50","50","","50"]
["","Напряжение","","","В","220-440","220-440","220-440","220-440","","220-240"]
["","Наименование","","","","","","","","","V1"]