{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXS-L1"]
[]
[]
[]
[]
["","","","FTXG25LV1BW / RXS25L3V1B1","FTXG35LV1BW / RXS35L3V1B1","FTXG50LV1BW / RXS50L2V1B1"]
["Холодопроизводительность","Ном.","kW","2.50 (1)","3.40 (1)","4.50 (1)"]
["Номинальная эффективность","EER","","4.30","3.87","3.58"]
["","COP","","4.10","3.72","3.58"]
["Теплопроизводительность","Ном.","kW","3.20 (2)","4.00 (2)","4.85 (2)"]
["Примечания","","","(1) - Температура в помещении: 27°CDB, 19°CWB; температура наружного воздуха: 35°CDB, 24°CWB","(1) - Температура в помещении: 27°CDB, 19°CWB; температура наружного воздуха: 35°CDB, 24°CWB","(1) - Температура в помещении: 27°CDB, 19°CWB; температура наружного воздуха: 35°CDB, 24°CWB"]
["","","","(2) - Температура в помещении: 20°CDB, 15°CWB; температура наружного воздуха: 7°CDB, 6°CWB.","(2) - Температура в помещении: 20°CDB, 15°CWB; температура наружного воздуха: 7°CDB, 6°CWB.","(2) - Температура в помещении: 20°CDB, 15°CWB; температура наружного воздуха: 7°CDB, 6°CWB."]