{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":9,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Холодопроизводительность","Ном.","","kW","4.00","4.00","5.20","4.00","6.00"]
["Номинальная эффективность","Annual energy consumption","","кВтч","467","471","593","457","787"]
["","EER","","","4.28","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","4.05","4.42","4.04","3.88"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A"]
["","","Нагрев","","A","A","A","A","A"]
["Теплопроизводительность","Ном.","","kW","4.60","6.80","6.80","6.50","7.80"]