{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / RZAG-A"]
[]
[]
[]
[]
["","","","","FTXM35N2V1B / RZAG35A2V1B","FTXM50N2V1B / RZAG35A2V1B","FTXM50N2V1B / RZAG50A2V1B","FTXM60N2V1B / RZAG50A2V1B","FTXM60N2V1B / RZAG60A2V1B","FTXM71N2V1B / RZAG60A2V1B"]
["Холодопроизводительность","Мин.","","kW","1.6","1.60","1.7","1.70","1.7","1.70"]
["","Макс.","","kW","5.0","5.00","6.0","6.00","6.8","6.80"]
["","Ном.","","kW","3.5","3.50","5.0","5.00","6.0","6.00"]
["Охлаждение помещений","SEER","","","7.70","7.76","7.41","7.53","6.90","6.90"]
["","Годовое потребление энергии","","кВтч/г","159","158","236","232","304","304"]
["","Производительность","Pрасч.","kW","3.50","3.50","5.00","5.00","6.00","6.00"]
["","Класс энергоэффективности","","","A++","A++","A++","A++","A++","A++"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","kW","2.60","2.60","4.50","4.50","4.60","4.50"]
["","SCOP/A","","","4.60","4.68","4.60","4.69","4.35","4.40"]
["","Класс энергоэффективности","","","A++","A++","A++","A++","A+","A+"]
["","Годовое потребление энергии","","кВтч/г","790","778","1,369","1,344","1,480","1,433"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","407","405","625","619","857","857"]
["","EER","","","4.30","4.32","4.00","4.04","3.50","3.50"]
["","COP","","","3.85","3.93","4.00","4.08","3.61","3.68"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A","A"]
["","","Нагрев","","A","A","A","A","A","A"]
["Теплопроизводительность","Ном.","","kW","4.00","4.00","6.00","6.00","7.00","7.00"]
["","Мин.","","kW","1.40","1.40","1.50","1.50","1.60","1.60"]
["","Макс.","","kW","5.30","5.30","6.50","6.50","7.50","7.50"]