{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F8"]
[]
[]
[]
[]
["","","","","FTXS71GV1B / RXS71FAV1B8"]
["Холодопроизводительность","Мин.","","кВт","2.3"]
["","Макс.","","кВт","8.5"]
["","Ном.","","кВт","7.10"]
["Подсоединение труб","Жидкость","НД","мм","6.35"]
["","Газ","НД","мм","15.9"]
["","Дренаж","OD","мм","18"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,175"]
["","EER","","","3.02"]
["","COP","","","3.22"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","B"]
["","","Нагрев","","C"]
["Теплопроизводительность","Ном.","","кВт","8.20"]
["","Мин.","","кВт","2.3"]
["","Макс.","","кВт","10.2"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - 220 В"]
["","","","","(3) - 230 В"]
["","","","","(4) - 240В"]
["","","","","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]