{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Тип","","","","","Воздухоочиститель"]
["Применение","","","","","Напольный тип"]
["Корпус","Цвет","","","","Front: White, Top/Side: Dark Grey"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","630"]
["","","","Ширина","мм","315"]
["","","","Глубина","мм","315"]
["Масса","Блок","","","кг","9.8"]
["Обслуживаемая площадь","м²","","","","62, 124"]
["CADR","м³/ч","","","","480"]
["Режим очистки воздуха","Входная мощность","","Turbo","кВт","0.080"]
["","","","M","кВт","0.016"]
["","","","L","кВт","0.011"]
["","","","Бесшумный","кВт","0.009"]
["Уровень звукового давления","Режим очистки воздуха","","Turbo","дБ(A)","55"]
["","","","Средн.","дБ(A)","34"]
["","","","Низк.","дБ(A)","25"]
["","","","Бесшумный","дБ(A)","19"]
["Вентилятор","Расход воздуха","Режим очистки воздуха","Turbo","м³/ч","480"]
["","","","Средний уровень","м³/ч","210"]
["","","","Низк.","м³/ч","132"]
["","","","Бесшумный","м³/ч","84"]
["Способ пылеудаления","","","","","Электростатический HEPA-фильтр"]
["Способ дезодорирования","","","","","Двойной стримерный разряд + дезодорирующий катализатор"]
["Стандартные аксессуары","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Шнур питания","м","","","","2"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50/60"]
["","Напряжение","","","V","220-240/220-230"]
["Примечания","","","","","(1) - Обслуживаемая площадь соответствует работе блока при максимальной скорости вентилятора (HH). Обслуживаемая площадь помещения — это пространство, из которого может быть удалено определенное количество частиц пыли за 30 минут."]
["","","","","","(2) - Преобразовано в стандарты NRCC на основе результатов испытаний в соответствии с JEM1467."]