{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","","","48"]
["","Охлаждение","","Выс.","дБA","","","48"]
["Стандартные аксессуары","Инструкции по установке","","","","","","1"]
["","Табличка с данными о заправке хладагентом","","","","","","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","","","1"]
["","Сливная пробка (только в моделях с тепловым насосом)","","","","","","1"]
["Хладагент","Charge","","","TCO2Eq","","","2.5"]
["","ПГП","","","","","","2,087.5"]
["","Заправка","","","кг","","","1.2"]
["","Тип","","","","","","R-410A"]
["Мотор вентилятора","Скорость вращения","Охлаждение","Самый низкий","об/мин","","","780"]
["","","Hагрев","Самый низкий","об/мин","","","740"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°C сух.т.","","","46"]
["","","","Мин.","°C сух.т.","","","-10"]
["","Hагрев","Темп. нар. возд.","Макс.","°CWB","","","18"]
["","","","Мин.","°CWB","","","-15"]
["Piping connections","Перепад уровней","IU - OU","Макс.","м","","","15"]
["","Дополнительная заправка хладагента","","","кг/м","","","0,02 (для длины труб свыше 10 м)"]
["Компрессор","Type","","","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","","","765"]
["","","","Глубина","мм","","","285"]
["","","","Высота","мм","","","550"]
["Масса","Блок","","","кг","","","34"]
["Вентилятор","Расход воздуха","Hагрев","Сверхнизкий","куб. фт/мин","","","904"]
["","","","Сверхнизкий","м³/мин","","","25.6"]
["","","Охлаждение","Сверхнизкий","м³/мин","","","30.1"]
["","","","Сверхнизкий","куб. фт/мин","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Частота","","","Гц","","","50"]
["","Напряжение","","","V","","","220-240"]
["Примечания","","","","","","","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","30.1","30.1"]
["","","Нагрев","Сверхнизкий","м³/мин","25.6","25.6"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","1063","1063"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","904","904"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550"]
["","","","Ширина","мм","765","765"]
["","","","Глубина","мм","285","285"]
["Масса","Блок","","","кг","34","34"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","780","780"]
["","","Нагревание","Самый низкий","об/мин","740","740"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10"]
["","","","Макс.","°C сух.т.","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15"]
["","","","Макс.","°CWB","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","46","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","47","47"]
["Хладагент","Тип","","","","R-410A","R-410A"]
["","Заправка","","","кг","1.0","1.0"]
["","Заправка","","","tCO2Eq","2.1","2.1"]
["","ПГП","","","","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]
["Примечания","","","","","(1) - 220 В"]
["","","","","","(2) - 230 В"]
["","","","","","(3) - 240В"]
["Стандартные аксессуары","Drain plug (only heat pump models)","","","","","1"]